1. Fixed the problem that the DSP FILTER switch cannot be stored when switching bands
2. Fixed the issue that the camera will enter the launch lock under certain circumstances when the internal battery is used for power supply
3. In DIGI mode, you can send preset messages by pressing the PTT of the fuselage;
    When sending a preset message, press PTT to terminate the transmission